HRR Comparison

|  |
| --- |
| HRR at different locations of the fire |

|  |  |  |
| --- | --- | --- |
| Location | Average HRR [MW] (20 s to 33 s) | Prescribed fire [MW] (HRRPUA 🞨 Area) |
| Floor fire | 5664 | 1759 kW 🞨 (31 m 🞨 100 m )= 5453 MW |
| Understory fire | 5374 | 1759 kW 🞨 (31 m 🞨 100 m )= 5453 MW |
| Canopy fire | 5352 | 1767 kW 🞨 (31 m 🞨 100 m )= 5478 MW |

|  |
| --- |
|  |
|  |
|  |
|  |
|  |
|  |

|  |
| --- |
|  |
|  |